**\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\***

**IOT Lab 04: Interfacing Sensors and Actuators with Raspberry Pi.**

**Roll No. BE051**

**\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\***

**Code:**

import RPi.GPIO as GPIO

import time

GPIO.setmode(GPIO.BCM)

GPIO.setup(12,GPIO.OUT)

p=GPIO.PWM(12,50)

p.start(7.5)

try:

while True:

p.ChangeDutyCycle(12.5)

time.sleep(4)

p.ChangeDutyCycle(2.5)

time.sleep(4)

except KeyboardInterrupt:

p.stop()

**Read.py**

#!/usr/bin/env python

import RPi.GPIO as GPIO

import SimpleMFRC522

reader = SimpleMFRC522.SimpleMFRC522()

try:

id, text = reader.read()

print(id)

print(text)

finally:

GPIO.cleanup()

**Write.py**

#!/usr/bin/env python

import RPi.GPIO as GPIO

import SimpleMFRC522

reader = SimpleMFRC522.SimpleMFRC522()

try:

text = raw\_input('New data:')

print("Now place your tag to write")

reader.write(text)

print("Written")


finally:


GPIO.cleanup()

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

**\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\***

**Photograph and Screenshots:**





\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*